;; net8192cu.inf 
;;
;; Realtek RTL8192C Wireless 802.11b/g/n USB 2.0 Network Adapter
;;
;; Copyright (C) 2009 Realtek Semiconductor Corp.
;;
;; This release is primarily for WHQL test.
;;

;FOR Vista

[Version]
Signature	= "$Windows NT$"
Class		= Net
ClassGUID	= {4d36e972-e325-11ce-bfc1-08002be10318}
Provider	= %Realtek%
CatalogFile.NT	= net8192cu.cat		;; for WHQL certified
DriverVer = 11/10/2010,1011.0.1110.2010

[Manufacturer]
%Realtek% = Realtek,NTamd64.6.0
%PCI% = PCI,NTamd64.6.0
%Sitecom% = Sitecom,NTamd64.6.0
%EDIMAX150% = EDIMAX150,NTamd64.6.0
%Abocom% = Abocom,NTamd64.6.0
%Amigo% = Amigo,NTamd64.6.0
%Hercules% = Hercules,NTamd64.6.0
%DLink% = DLink,NTamd64.6.0
%Belkin% = Belkin,NTamd64.6.0
%PlanexAbocom88cu% = PlanexAbocom88cu,NTamd64.6.0
%Zyxel% = Zyxel,NTamd64.6.0
%EDIMAX300% = EDIMAX300,NTamd64.6.0
%PlanexAbocom92cu% = PlanexAbocom92cu,NTamd64.6.0
%Abocom92cu% = Abocom92cu,NTamd64.6.0
%ATKK92cu% = ATKK92cu,NTamd64.6.0
%TRENDnet88cus% = TRENDnet88cus,NTamd64.6.0
%AZ88vau% = AZ88vau,NTamd64.6.0
%AZ88vau_G% = AZ88vau_G,NTamd64.6.0
%AZ88cus% = AZ88cus,NTamd64.6.0
%Feixun92cu% = Feixun92cu,NTamd64.6.0

[ControlFlags]
ExcludeFromSelect = *

;;****************************************************************************
;; IDs for X86
;;****************************************************************************
[Realtek.NTx86.6.0]
%RTL8188cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_8176								; RTK 88CU board for B/G/N      
%RTL8188cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_8176&REV_0200&SS                                                   
%RTL8188cu_G.DeviceDesc% = RTL8192cu_G.ndi, USB\VID_0BDA&PID_8177							; RTK 88CU board for B/G        ; RTK demo board for B/G
%RTL8188cu_G.DeviceDesc% = RTL8192cu_G.ndi, USB\VID_0BDA&PID_8177&REV_0200&SS                                                 
%RTL8188ce_vau.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_8170                           ; RTK 88CE_VAU board for B/G/N  
%RTL8188ce_vau.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_8170&REV_0200&SS                                               
%RTL8188ce_vau_G.DeviceDesc% = RTL8192cu_G.ndi, USB\VID_0BDA&PID_817E                       ; RTK 88CE_VAU board for B/G    
%RTL8188ce_vau_G.DeviceDesc% = RTL8192cu_G.ndi, USB\VID_0BDA&PID_817E&REV_0200&SS                                             
%RTL8192ce_vau.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_817C                           ; RTK 92CE_VAU board for B/G/N  
%RTL8192ce_vau.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_817C&REV_0200&SS                                               
%RTL8188cu_slim_solo.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_817A                     ; RTK slim_solo board for B/G/N 
%RTL8188cu_slim_solo.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_817A&REV_0200&SS                                         
%RTL8188cu_slim_combo.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_817B                    ; RTK slim_combo board for B/G/N
%RTL8188cu_slim_combo.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_817B&REV_0200&SS                                        
%RTL8188ru.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_817F                               ; RTK 88RU board for B/G/N      
%RTL8188ru.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_817F&REV_0200&SS                                                   
%RTL8188cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_103C&PID_1629	; HP/Liteon                 ; HP/Liteon board for B/G/N     
%RTL8192cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_8192                                                               
%RTL8192cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_8178                               ; RTK 92CU board for B/G/N      
%RTL8723u.DeviceDesc%  = RTL8723u.ndi, USB\VID_0BDA&PID_8724
%RTL8723u.DeviceDesc%  = RTL8723u.ndi, USB\VID_0BDA&PID_8724&MI_02


[PCI.NTx86.6.0]
%PCI.DeviceDesc% = RTL8192cu.ndi, USB\VID_2019&PID_ED17

[Sitecom.NTx86.6.0]
%Sitecom.DeviceDesc% = RTL8192cu.ndi, USB\VID_0DF6&PID_0052

[EDIMAX150.NTx86.6.0]
%EDIMAX150.DeviceDesc% = RTL8192cu.ndi, USB\VID_7392&PID_7811

[Abocom.NTx86.6.0]
%Abocom.DeviceDesc% = RTL8192cu.ndi, USB\VID_07B8&PID_8189

[Amigo.NTx86.6.0]
%Amigo.DeviceDesc% = RTL8192cu.ndi, USB\VID_0EB0&PID_9071

[Hercules.NTx86.6.0]
%Hercules.DeviceDesc% = RTL8192cu.ndi, USB\VID_06F8&PID_E033

[DLink.NTx86.6.0]
%DLink-1.DeviceDesc% = RTL8192cu.ndi, USB\VID_2001&PID_330A
%DLink-2.DeviceDesc% = RTL8192cu.ndi, USB\VID_2001&PID_3309
%DLink-3.DeviceDesc% = RTL8192cu.ndi, USB\VID_2001&PID_3308

[Belkin.NTx86.6.0]
%Belkin.DeviceDesc% = Belkin.ndi, USB\VID_050D&PID_1102

[PlanexAbocom88cu.NTx86.6.0]
%PlanexAbocom88cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_2019&PID_AB2A

[Zyxel.NTx86.6.0]
%Zyxel.DeviceDesc% = RTL8192cu.ndi, USB\VID_0586&PID_341F

[EDIMAX300.NTx86.6.0]
%EDIMAX300.DeviceDesc% = RTL8192cu.ndi, USB\VID_7392&PID_7822

[PlanexAbocom92cu.NTx86.6.0]
%PlanexAbocom92cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_2019&PID_AB2B

[Abocom92cu.NTx86.6.0]
%Abocom92cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_07B8&PID_8178

[ATKK92cu.NTx86.6.0]
%ATKK92cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_07AA&PID_0056

[TRENDnet88cus.NTx86.6.0]
%TRENDnet88cus.DeviceDesc% = RTL8192cu.ndi, USB\VID_20F4&PID_648B

[AZ88vau.NTx86.6.0]
%AZ88vau.DeviceDesc% = RTL8192cu.ndi, USB\VID_13D3&PID_3358						; AZ 88CE_VAU for B/G/N

[AZ88vau_G.NTx86.6.0]
%AZ88vau_G.DeviceDesc% = RTL8192cu_G.ndi, USB\VID_13D3&PID_3359					; AZ 88CE_VAU for B/G

[AZ88cus.NTx86.6.0]
%AZ88cus.DeviceDesc% = RTL8192cu_G.ndi, USB\VID_13D3&PID_3357				; AZ 88CUS for B/G/N

[Feixun92cu.NTx86.6.0]
%Feixun92cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_4855&PID_0090				; Feixun 88CUS for B/G/N
%Feixun92cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_4855&PID_0091				; Feixun 92CU for B/G/N

;;****************************************************************************
;; IDs for X64
;;****************************************************************************
[Realtek.NTamd64.6.0]
%RTL8188cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_8176								; RTK 88CU board for B/G/N      
%RTL8188cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_8176&REV_0200&SS                                                   
%RTL8188cu_G.DeviceDesc% = RTL8192cu_G.ndi, USB\VID_0BDA&PID_8177							; RTK 88CU board for B/G        ; RTK demo board for B/G
%RTL8188cu_G.DeviceDesc% = RTL8192cu_G.ndi, USB\VID_0BDA&PID_8177&REV_0200&SS                                                 
%RTL8188ce_vau.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_8170                           ; RTK 88CE_VAU board for B/G/N  
%RTL8188ce_vau.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_8170&REV_0200&SS                                               
%RTL8188ce_vau_G.DeviceDesc% = RTL8192cu_G.ndi, USB\VID_0BDA&PID_817E                       ; RTK 88CE_VAU board for B/G    
%RTL8188ce_vau_G.DeviceDesc% = RTL8192cu_G.ndi, USB\VID_0BDA&PID_817E&REV_0200&SS                                             
%RTL8192ce_vau.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_817C                           ; RTK 92CE_VAU board for B/G/N  
%RTL8192ce_vau.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_817C&REV_0200&SS                                               
%RTL8188cu_slim_solo.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_817A                     ; RTK slim_solo board for B/G/N 
%RTL8188cu_slim_solo.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_817A&REV_0200&SS                                         
%RTL8188cu_slim_combo.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_817B                    ; RTK slim_combo board for B/G/N
%RTL8188cu_slim_combo.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_817B&REV_0200&SS                                        
%RTL8188ru.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_817F                               ; RTK 88RU board for B/G/N      
%RTL8188ru.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_817F&REV_0200&SS                                                   
%RTL8188cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_103C&PID_1629	; HP/Liteon                 ; HP/Liteon board for B/G/N     
%RTL8192cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_8192                                                               
%RTL8192cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_8178                               ; RTK 92CU board for B/G/N      
%RTL8192cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_0586&PID_341F	; Zyxel/Abocom
%RTL8723u.DeviceDesc%  = RTL8723u.ndi, USB\VID_0BDA&PID_8724
%RTL8723u.DeviceDesc%  = RTL8723u.ndi, USB\VID_0BDA&PID_8724&MI_02
 
[PCI.NTamd64.6.0]
%PCI.DeviceDesc% = RTL8192cu.ndi, USB\VID_2019&PID_ED17

[Sitecom.NTamd64.6.0]
%Sitecom.DeviceDesc% = RTL8192cu.ndi, USB\VID_0DF6&PID_0052

[EDIMAX150.NTamd64.6.0]
%EDIMAX150.DeviceDesc% = RTL8192cu.ndi, USB\VID_7392&PID_7811

[Abocom.NTamd64.6.0]
%Abocom.DeviceDesc% = RTL8192cu.ndi, USB\VID_07B8&PID_8189

[Amigo.NTamd64.6.0]
%Amigo.DeviceDesc% = RTL8192cu.ndi, USB\VID_0EB0&PID_9071

[Hercules.NTamd64.6.0]
%Hercules.DeviceDesc% = RTL8192cu.ndi, USB\VID_06F8&PID_E033

[DLink.NTamd64.6.0]
%DLink-1.DeviceDesc% = RTL8192cu.ndi, USB\VID_2001&PID_330A
%DLink-2.DeviceDesc% = RTL8192cu.ndi, USB\VID_2001&PID_3309
%DLink-3.DeviceDesc% = RTL8192cu.ndi, USB\VID_2001&PID_3308

[Belkin.NTamd64.6.0]
%Belkin.DeviceDesc% = Belkin.ndi, USB\VID_050D&PID_1102

[PlanexAbocom88cu.NTamd64.6.0]
%PlanexAbocom88cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_2019&PID_AB2A

[Zyxel.NTamd64.6.0]
%Zyxel.DeviceDesc% = RTL8192cu.ndi, USB\VID_0586&PID_341F

[EDIMAX300.NTamd64.6.0]
%EDIMAX300.DeviceDesc% = RTL8192cu.ndi, USB\VID_7392&PID_7822

[PlanexAbocom92cu.NTamd64.6.0]
%PlanexAbocom92cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_2019&PID_AB2B

[Abocom92cu.NTamd64.6.0]
%Abocom92cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_07B8&PID_8178

[ATKK92cu.NTamd64.6.0]
%ATKK92cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_07AA&PID_0056

[TRENDnet88cus.NTamd64.6.0]
%TRENDnet88cus.DeviceDesc% = RTL8192cu.ndi, USB\VID_20F4&PID_648B

[AZ88vau.NTamd64.6.0]
%AZ88vau.DeviceDesc% = RTL8192cu.ndi, USB\VID_13D3&PID_3358					; AZ 88CE_VAU for B/G/N

[AZ88vau_G.NTamd64.6.0]
%AZ88vau_G.DeviceDesc% = RTL8192cu_G.ndi, USB\VID_13D3&PID_3359				; AZ 88CE_VAU for B/G

[AZ88cus.NTamd64.6.0]
%AZ88cus.DeviceDesc% = RTL8192cu_G.ndi, USB\VID_13D3&PID_3357				; AZ 88CUS for B/G/N

[Feixun92cu.NTamd64.6.0]
%Feixun92cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_4855&PID_0090				; Feixun 88CUS for B/G/N
%Feixun92cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_4855&PID_0091				; Feixun 92CU for B/G/N

;;****************************************************************************
;; Windows 2000/XP
;;****************************************************************************
;;----------------------------------------------------------------------------
;; Realtek default installation
;;----------------------------------------------------------------------------
[RTL8192cu.ndi.NT]
AddReg			= RTL8192cu.nt5.reg, RTL8192cu.common.reg, RTLWLAN.reg, 11nWirelessMode.reg
Characteristics		= 0x84
BusType			= 15 
CopyFiles			= RTL8192cu.CopyFiles
*IfType			= 71            ; IF_TYPE_IEEE80211
*MediaType		= 16            ; NdisMediumNative802_11
*PhysicalMediaType		= 9          	; NdisPhysicalMediumNative802_11

[RTL8192cu.ndi.NT.Services]
AddService		= RTL8192cu, 2, RTL8192cu.nt5.Service, RTL8192cu.nt5.EventLog

;;----------------------------------------------------------------------------
;; Realtek G mode sku installation
;;----------------------------------------------------------------------------
[RTL8192cu_G.ndi.NT]
AddReg			= RTL8192cu.nt5.reg, RTL8192cu.common.reg, RTLWLAN.reg, 11gWirelessMode.reg
Characteristics		= 0x84
BusType			= 15 
CopyFiles			= RTL8192cu.CopyFiles
*IfType			= 71            ; IF_TYPE_IEEE80211
*MediaType		= 16            ; NdisMediumNative802_11
*PhysicalMediaType		= 9          	; NdisPhysicalMediumNative802_11

[RTL8192cu_G.ndi.NT.Services]
AddService		= RTL8192cu, 2, RTL8192cu.nt5.Service, RTL8192cu.nt5.EventLog

;;----------------------------------------------------------------------------
;; Realtek 8723u default installation
;;----------------------------------------------------------------------------
[RTL8723u.ndi.NT]
AddReg			= RTL8192cu.nt5.reg, RTL8723u.common.reg, RTLWLAN.reg
Characteristics		= 0x84
BusType			= 15 
CopyFiles		= RTL8192cu.CopyFiles
*IfType			= 71            ; IF_TYPE_IEEE80211
*MediaType		= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          	; NdisPhysicalMediumNative802_11

[RTL8723u.ndi.NT.Services]
AddService		= RTL8192cu, 2, RTL8192cu.nt5.Service, RTL8192cu.nt5.EventLog

;;----------------------------------------------------------------------------
;; Belkin customized installation
;;----------------------------------------------------------------------------
[Belkin.ndi.NT]
AddReg			= RTL8192cu.nt5.reg, RTL8192cu.common.reg, RTLWLAN.reg, Belkin.reg
Characteristics		= 0x84
BusType			= 15 
CopyFiles			= RTL8192cu.CopyFiles
*IfType			= 71            ; IF_TYPE_IEEE80211
*MediaType		= 16            ; NdisMediumNative802_11
*PhysicalMediaType		= 9          	; NdisPhysicalMediumNative802_11

[Belkin.ndi.NT.Services]
AddService		= RTL8192cu, 2, RTL8192cu.nt5.Service, RTL8192cu.nt5.EventLog


;;****************************************************************************
;; Windows 2000/XP parameters
;;****************************************************************************
[RTL8192cu.nt5.reg]
HKR, Ndi\Interfaces,	UpperRange, 0, "ndis5,mdcwifi"
HKR, Ndi\Interfaces,	LowerRange, 0, "wlan, ethernet"
HKR, Ndi,		Service,    0, "RTL8192cu"

[RTL8192cu.nt5.Service]
DisplayName    = %RTL8192cu.DeviceDesc.DispName%
ServiceType    = 1		; %SERVICE_KERNEL_DRIVER%
StartType      = 3		; %SERRVICE_DEMAND_START%
ErrorControl   = 1		; %SERRVICE_ERROR_NORMAL%
ServiceBinary  = %12%\RTL8192cu.sys
LoadOrderGroup = NDIS

[RTL8192cu.nt5.EventLog]
AddReg = RTL8192cu.nt5.AddEventLog.reg

[RTL8192cu.nt5.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported  , 0x00010001, 7

;*******************************************************************************
; RTL8192cu common paramters
;*******************************************************************************
[RTL8192cu.common.reg]
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

HKR,defaults,WiFi11bIbss,0,"0"
HKR,,WiFi11bIbss,0,"0"

HKR,defaults,bRateAdaptive,0,"1"
HKR,,bRateAdaptive,0,"1"

HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"

HKR,defaults,WiFiConfg,0,"0"
HKR,,WiFiConfg,0,"0"

HKR,defaults,CcxRm,0,"1"
HKR,,CcxRm,0,"1"

HKR,defaults,CcxOffLineDurUpLimit,0,"0"
HKR,,CcxOffLineDurUpLimit,0,"0"

;; For USB selective suspend.
HKR,,EnableUsbSS,0,"0"

;; For GPIO detect setting.
HKR,,TimerGPIO,0,"0"
HKR,,GPIODelay,0,"1000"
HKR,,GPIOBack,0,"1000"

;; For PDN mode switch.
HKR,,PDNMode,0,"0"

;; For PDN mode switch.
HKR,,DongleSS,0,"1"

;; For Different selective suspend power save level. Now support 1 and 2. 2 is better.
HKR,,SSPwrLvl,0,"2"

;*******************************************************************************
; RTL8723u common paramters
;*******************************************************************************
[RTL8723u.common.reg]
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

HKR,defaults,WiFi11bIbss,0,"0"
HKR,,WiFi11bIbss,0,"0"

HKR,defaults,bRateAdaptive,0,"1"
HKR,,bRateAdaptive,0,"1"

HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"

HKR,defaults,WiFiConfg,0,"0"
HKR,,WiFiConfg,0,"0"

HKR,defaults,CcxRm,0,"1"
HKR,,CcxRm,0,"1"

HKR,defaults,CcxOffLineDurUpLimit,0,"0"
HKR,,CcxOffLineDurUpLimit,0,"0"

;; For USB selective suspend.
HKR,,EnableUsbSS,0,"0"

;; For GPIO detect setting.
HKR,,TimerGPIO,0,"0"
HKR,,GPIODelay,0,"1000"
HKR,,GPIOBack,0,"1000"

;; For PDN mode switch.
HKR,,PDNMode,0,"1"

;; For PDN mode switch.
HKR,,DongleSS,0,"1"

;;----------------------------------------------------------------------------
;; Realtek WLAN NIC parameters
;;----------------------------------------------------------------------------
[RTLWLAN.reg]
HKR,defaults,SSID,0,"ANY"
HKR,,SSID,0,"ANY"

HKR,defaults,Channel,0,"1"
HKR,,Channel,0,"1"

HKR,Ndi\params\NetworkType,			ParamDesc,  0, %NETWORK_TYPE_STR%
HKR,Ndi\params\NetworkType,			type,       0, "enum"
HKR,Ndi\params\NetworkType,			default,    0, "1"
HKR,Ndi\params\NetworkType\enum,		"0",        0, %AD_HOC_STR%
HKR,Ndi\params\NetworkType\enum,		"1",        0, %INFRASTRUCTURE_STR%
HKR,Ndi\params\NetworkType\enum,		"2",        0, %AUTO_SELECT%
HKR,defaults,NetworkType,0,"1"
HKR,,NetworkType,0,"1"

HKR,defaults,StaUapsd,0,"0"
HKR,,StaUapsd,0,"0"

; For B/G mode and B/G/N mode switch, we will use different wireless mode registry in later section
;HKR,Ndi\params\WirelessMode, 			ParamDesc, 	0, %WL_MODE_STR%
;HKR,Ndi\params\WirelessMode, 			type, 		0, "enum"
;HKR,Ndi\params\WirelessMode, 			default, 	0, "8"
;HKR,Ndi\params\WirelessMode\enum, 		"2", 		0, %IEEE_802_11B_STR%
;HKR,Ndi\params\WirelessMode\enum, 		"4", 		0, %IEEE_802_11BG_STR%
;HKR,Ndi\params\WirelessMode\enum, 		"8", 		0, %IEEE_802_11BGN_STR%
;HKR,defaults,WirelessMode, 0, "8"
;HKR,,WirelessMode, 0, "8"

HKR,defaults,RxReorder,0,"1"
HKR,,RxReorder,0,"1"

HKR,,DefaultKeyID,,"0"
HKR,,DefaultKey0,,""
HKR,,DefaultKey1,,""
HKR,,DefaultKey2,,""
HKR,,DefaultKey3,,""

;Inactive Power Save
HKR,defaults,InactivePs,0,"2"
HKR,,InactivePs,0,"2"

;Leisure Power Save
HKR,defaults,bLeisurePs,0,"2"
HKR,,bLeisurePs,0,"2"

;Fw Control LPS
HKR,defaults,bFwCtrlLPS,0,"3"
HKR,,bFwCtrlLPS,0,"3"

;; LPS Interval
;HKR,defaults,LPSIntvl,0,"5"
HKR,,LPSIntvl,0,"5"

; Reset Tx Hang
HKR,defaults,USBResetTxHang,0,"1"
HKR,,USBResetTxHang,0,"1"

HKR,,WEPinNmode,0,"0"

;-------------------------------------------------------------------------------
;	USB Tx/Rx aggregation
;-------------------------------------------------------------------------------

HKR,defaults,UsbRxAggMode,0,"3"
HKR,,UsbRxAggMode,0,"3"

HKR,defaults,UsbRxAggBlockCount,0,"8"
HKR,,UsbRxAggBlockCount,0,"8"

HKR,defaults,UsbRxAggBlockTimeout,0,"6"
HKR,,UsbRxAggBlockTimeout,0,"6"

HKR,defaults,UsbRxAggPageCount,0,"16"
HKR,,UsbRxAggPageCount,0,"16"

HKR,defaults,UsbRxAggPageTimeout,0,"6"
HKR,,UsbRxAggPageTimeout,0,"6"

HKR,defaults,UsbTxAggMode,0,"1"
HKR,,UsbTxAggMode,0,"1"

HKR,defaults,UsbTxAggDescNum,0,"6"
HKR,,UsbTxAggDescNum,0,"6"

;;----------------------------------------------------------------------------
;; Belkin WLAN NIC parameters
;;----------------------------------------------------------------------------
[Belkin.reg]
HKR,Ndi\params\RFOff,			ParamDesc,  0, "Radio"
HKR,Ndi\params\RFOff,			type,       0, "enum"
HKR,Ndi\params\RFOff,			default,    0, "0"
HKR,Ndi\params\RFOff\enum,		"0",        0, "On"
HKR,Ndi\params\RFOff\enum,		"1",        0, "Off"
HKR,defaults,RFOff,0,"0"
HKR,,RFOff,0,"0"

;;----------------------------------------------------------------------------
;; Wireless mode option parameters
;;----------------------------------------------------------------------------
[11gWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,defaults,WirelessMode, 0, "4"
HKR,,WirelessMode, 0, "4"

[11nWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,Ndi\params\WirelessMode\enum, 	"8", 		0, %IEEE_802_11BGN_STR%
HKR,defaults,WirelessMode, 0, "8"
HKR,,WirelessMode, 0, "8"


;*******************************************************************************
; Destination Directory
;*******************************************************************************
[RTL8192cu.CopyFiles]
RTL8192cu.sys,,,2

[DestinationDirs]
DefaultDestDir     = 11
RTL8192cu.CopyFiles		= 12

;;****************************************************************************
;; Source Files
;;****************************************************************************
[SourceDisksFiles]
RTL8192cu.sys = 1

[SourceDisksNames]
1=%DISKNAME%,,,

;*******************************************************************************
; Strings
;*******************************************************************************
[Strings]
SSID_STR					= "SSID"
CHANNEL_STR				= "Channel"
NETWORK_TYPE_STR			= "Network Type"
LED_CONTROL_STR				= "LED Control" 
POWER_SAVE_STR				= "Power Save Mode"
WIFI_IBSS_STR				= "IBSS Default 11b Mode"
RATE_ADAPTIVE_STR			= "Rate Adaptive"
QOS_STR					= "QoS"
WiFiConfg_STR	  			= "WiFiConfg"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX Radio Measurement"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX Max Off-Line Measurement (0: unlimited)"
FORCE_PRIORITY_STR			= "Forced Priority"
HW_PARA_STR				= "Init from HwParaFile"
THREE_WIRE_MODE_STR			= "Three Wire Programming Mode"
BOARD_TYPE_STR				= "Board Type"
PROTECTION_MODE_STR			= "Protection Mode"
TPC_STR					= "Transmit Power Control"
TPC_POLARITY_STR				= "TPC Polarity Select"
HIGH_POWER_STR				= "High Power Mechanism"
INIT_GAIN_STR				= "Initial Gain State"
CW_MAX_MIN_STR				= "Contention Window"
PSP_XLINK_STR				= "PSP XLink Mode"
DISABLE_STR				= "Disable"
ENABLE_STR				= "Enable"
AD_HOC_STR				= "Ad Hoc"
INFRASTRUCTURE_STR			= "Infrastructure"
AUTO_SELECT				= "Auto select"
WL_MODE_STR				= "Wireless Mode"
RX_REORDER_STR				= "Rx Reorder"
CAM_STR					= "CAM"
MAX_PSP_STR				= "MAX_PSP"
Fast_PSP_STR				= "Fast_PSP"
NO_AC_STR				= "No AC (Disable)"
ALL_AC_STR				= "ALL AC"
IEEE_802_11B_STR 				= "IEEE 802.11b"
IEEE_802_11BG_STR 				= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"

;-------------------------------------------------------------------------------
;	USB Tx/Rx aggregation strings
;-------------------------------------------------------------------------------
RX_AGG_MODE_STR				= "Rx Aggregation Mode"
RX_AGG_MODE_BLOCK_STR			= "Rx Agg USB Block Mode"
RX_AGG_MODE_PAGE_STR			= "Rx Agg DMA Page Mode"
RX_AGG_MODE_MIXED_STR			= "Rx Agg USB and Page Mixed Mode"
RX_AGG_USB_BLOCK_STR			= "Rx Agg USB Block Threshold"
RX_AGG_USB_TIMEOUT_STR			= "Rx Agg USB Timeout"
RX_AGG_DMA_PAGE_STR			= "Rx Agg DMA Page Threshold"
RX_AGG_DMA_TIMEOUT_STR			= "Rx Agg DMA Timeout"
TX_AGG_MODE_STR				= "Tx Aggregation Mode"
TX_AGG_DESC_PER_OUT_STR			= "Tx Agg Number of descriptor per bulk out"

;*******************************************************************************
; manufacture description
;*******************************************************************************
Realtek					= "Realtek Semiconductor Corp."
PCI             		= "PLANEX COMMUNICATIONS INC"
Sitecom         		= "Sitecom Europe B.V."
EDIMAX150         		= "EDIMAX"
Abocom					= "AboCom System, Inc."
Amigo					= "Amigo Technology Inc"
Hercules				= "Guillemot Corporation S.A"
DLink					= "D-Link Corporation"
Belkin					= "Belkin International, Inc."
PlanexAbocom88cu		= "PLANEX COMMUNICATIONS INC."
Zyxel					= "ZyXEL"
EDIMAX300         		= "EDIMAX "
PlanexAbocom92cu		= "PLANEX COMMUNICATIONS INC. "
Abocom92cu				= "AboCom System, Inc. "
ATKK92cu				= "Allied Telesis K.K."
TRENDnet88cus			= "TRENDnet"
AZ88vau					= "Realtek Semiconductor Corp. "
AZ88vau_G				= "Realtek Semiconductor Corp.  "
AZ88cus					= "Realtek Semiconductor Corp.   "
Feixun92cu				= "Shanghai Feixun Communication Co.,Ltd"

;*******************************************************************************
;	Source disk name
;*******************************************************************************
DISKNAME				= "Realtek RTL8192CU Wireless LAN 802.11n USB 2.0 Network Adapter Driver Disk"
RTL8192cu.DeviceDesc 			= "Realtek RTL8192CU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8192cu.DeviceDesc.DispName		= "Realtek RTL8192CU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8188cu.DeviceDesc 			= "Realtek RTL8188CU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8188cu.DeviceDesc.DispName		= "Realtek RTL8188CU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8188cu_G.DeviceDesc 			= "Realtek RTL8188CU Wireless LAN 802.11 USB 2.0 Network Adapter"
RTL8188cu_G.DeviceDesc.DispName		= "Realtek RTL8188CU Wireless LAN 802.11 USB 2.0 Network Adapter"
RTL8188ce_vau.DeviceDesc 		= "Realtek RTL8188CE-VAU Wireless LAN 802.11n USB minicard"
RTL8188ce_vau.DeviceDesc.DispName	= "Realtek RTL8188CE-VAU Wireless LAN 802.11n USB minicard"
RTL8188ce_vau_G.DeviceDesc 		= "Realtek RTL8188CE-VAU Wireless LAN 802.11 USB minicard"
RTL8188ce_vau_G.DeviceDesc.DispName	= "Realtek RTL8188CE-VAU Wireless LAN 802.11 USB minicard"
RTL8192ce_vau.DeviceDesc 		= "Realtek RTL8192CE-VAU Wireless LAN 802.11n USB minicard"
RTL8192ce_vau.DeviceDesc.DispName	= "Realtek RTL8192CE-VAU Wireless LAN 802.11n USB minicard"
RTL8188cu_slim_solo.DeviceDesc		= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Solo"
RTL8188cu_slim_solo.DeviceDesc.DispName	= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Solo"
RTL8188cu_slim_combo.DeviceDesc		= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Combo"
RTL8188cu_slim_combo.DeviceDesc.DispName= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Combo"
RTL8188ru.DeviceDesc 			= "Realtek RTL8188RU Wireless LAN 802.11n USB High Power Dongle"
RTL8188ru.DeviceDesc.DispName		= "Realtek RTL8188RU Wireless LAN 802.11n USB High Power Dongle"
PCI.DeviceDesc 					= "GW-USValue-EZ"
PCI.DeviceDesc.DispName			= "GW-USValue-EZ"
Sitecom.DeviceDesc 			= "Sitecom Wireless Ultra Nano USB Adapter 150N X1 WL-365"
Sitecom.DeviceDesc.DispName		= "Sitecom Wireless Ultra Nano USB Adapter 150N X1 WL-365"
EDIMAX150.DeviceDesc 			= "150Mbps Wireless 802.11b/g/n Nano USB Adapter"
EDIMAX150.DeviceDesc.DispName		= "150Mbps Wireless 802.11b/g/n Nano USB Adapter"
Abocom.DeviceDesc 			= "802.11n/b/g Mini Wireless LAN USB2.0 Adapter"
Abocom.DeviceDesc.DispName		= "802.11n/b/g Mini Wireless LAN USB2.0 Adapter"
Amigo.DeviceDesc 			= "Wireless USB Card"
Amigo.DeviceDesc.DispName		= "Wireless USB Card"
Hercules.DeviceDesc 			= "Hercules Wireless N Pico USB "
Hercules.DeviceDesc.DispName		= "Hercules Wireless N Pico USB "
DLink-1.DeviceDesc 			= "D-Link DWA-133 Wireless N USB Adapter"
DLink-1.DeviceDesc.DispName		= "D-Link DWA-133 Wireless N USB Adapter"
DLink-2.DeviceDesc 			= "D-Link DWA-135 Wireless N USB Adapter"
DLink-2.DeviceDesc.DispName		= "D-Link DWA-135 Wireless N USB Adapter"
DLink-3.DeviceDesc 			= "D-Link DWA-121 Wireless N USB Adapter"
DLink-3.DeviceDesc.DispName		= "D-Link DWA-121 Wireless N USB Adapter"
Belkin.DeviceDesc 			= "Surf Wireless Micro USB Adapter"
Belkin.DeviceDesc.DispName		= "Surf Wireless Micro USB Adapter"
PlanexAbocom88cu.DeviceDesc 		= "GW-USNano2"
PlanexAbocom88cu.DeviceDesc.DispName	= "GW-USNano2"
ZyXEL.DeviceDesc 			= "ZyXEL Wireless LAN 802.11n USB 2.0 Network Adapter"
ZyXEL.DeviceDesc.DispName		= "ZyXEL Wireless LAN 802.11n USB 2.0 Network Adapter"
EDIMAX300.DeviceDesc 			= "Edimax 300Mbps wireless 802.11b/g/n USB adapter"
EDIMAX300.DeviceDesc.DispName		= "Edimax 300Mbps wireless 802.11b/g/n USB adapter"
PlanexAbocom92cu.DeviceDesc 		= "GW-USEco300"
PlanexAbocom92cu.DeviceDesc.DispName	= "GW-USEco300"
Abocom92cu.DeviceDesc			= "802.11n/b/g Mini Wireless LAN USB2.0 Adapter"
Abocom92cu.DeviceDesc.DispName		= "802.11n/b/g Mini Wireless LAN USB2.0 Adapter"
ATKK92cu.DeviceDesc			= "Corega CG-WLUSB300NS"
ATKK92cu.DeviceDesc.DispName		= "Corega CG-WLUSB300NS"
TRENDnet88cus.DeviceDesc		= "TRENDnet 150Mbps Micro Wireless N USB Adapter"
TRENDnet88cus.DeviceDesc.DispName	= "TRENDnet 150Mbps Micro Wireless N USB Adapter"
AZ88vau.DeviceDesc			= "Realtek RTL8188CE-VAU Wireless LAN 802.11n USB minicard"
AZ88vau.DeviceDesc.DispName		= "Realtek RTL8188CE-VAU Wireless LAN 802.11n USB minicard"
AZ88vau_G.DeviceDesc			= "Realtek RTL8188CE-VAU Wireless LAN 802.11 USB minicard"
AZ88vau_G.DeviceDesc.DispName		= "Realtek RTL8188CE-VAU Wireless LAN 802.11 USB minicard"
AZ88cus.DeviceDesc				= "Wireless USB Card"
AZ88cus.DeviceDesc.DispName		= "Wireless USB Card"
Feixun92cu.DeviceDesc 			= "FEIXUN Wireless LAN 802.11n USB 2.0 Network Adaptor"
Feixun92cu.DeviceDesc.DispName		= "FEIXUN Wireless LAN 802.11n USB 2.0 Network Adaptor"
RTL8723u.DeviceDesc 			= "Realtek RTL8723U Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8723u.DeviceDesc.DispName		= "Realtek RTL8723U Wireless LAN 802.11n USB 2.0 Network Adapter"
