|  |  |  |
| --- | --- | --- |
| 000A0  Version（custom） | 000A1  Display inward character string（custom） | 000A2  Display series number（custom） |
| 000B0  Factory Default |  | 000600  PS2 |
| 000601  RS-232 | 000602  USB-HID |  |
|  |  |  |
| 013300  Default Scan Mode | 013301  Single not triggered  Not：CCD inapplicability | 013302  Key Delay  No：CCD inapplicability |
| 013303  Key Delay not triggered  Not：CCD inapplicability | 013304  Continuous Scan Mode | 013305  Auto flashing |
| 014201  Sound On  Default | 014200  Sound Off |  |
| 014300  High Volume Sound | 014301  Low Volume Sound |  |
| 01400  Code ID Off  default | 01401  Code ID On | 01402  Rear Code ID On |
| 0005000  English  Default | 0005001  Canada-French | 0005002  Netherlands-Dutch |
| 0005003  Spain-Spanish | 0005004  Argentina-Latin American | 0005005  Brazil-Portuguese |
| 0005006  Denmark-Danish | 0005007  UK-English | 0005008  Italy-Italian |
| 0005009  France-French | 0005010  Germany-German | 0005011  Norway-Northern Sami |
| 0005012  Sweden,Finland-Swedish,Finnish | 0005013  Slovakia-Slovak | 0005014  Portuguesa-Portuguese |
| 0005015  Czech Republic-Czech | 0005016  Belgium -Dutch | 0005017  Turkey-F |
| 0005018  Turkey-Q | 0005019  Poland-Polish | 0005020  Switzerland –German,French |
| 0005021  Croatia-Srb-Crt | 0005022  Hungary -Hungarian | 0005023  Japan-Japanese |
| 0005024  Russia-Russian |  |  |
| 000701  Baudrate600bps | 000702  Baudrate1200bps | 000703  Baudrate2400bps |
| 000704  Baudrate4800bps | 000705  Baudrate9600bps  Default | 000706  Baudrate19200bps |
| 000707  Baudrate38400bps | 000708  Baudrate57600bps | 000709  Baudrate115200bps |
| 001200  Serial Port no Check | 001201  Serial port :XON/OFF | 001202  Serial port:RTS/CTS |
| 001203  Serial port:ACK/NAK | 0013020  Serial port handshake timeout 2S | 0013050  Serial port handshake timeout 5S |
| 001500  Fastest transmit rate | 001502  Medium transmit rate Default | 001504  Lower transmit rate |
| 001506  Lowest transmit rate | 00161  Forward image identifyDefault | 00160  Reverse image identify |
| 00221  Enable code39 | 00220  Disable code39 | 0031m  code39 IDAs m |
| 00231  Enable code39FullASCII  Default | 00230  Disable code39 FullASCII | 00240  Disable code39 MOD43Check  Default |
| 00241  Enable code39 MOD43Check | 00251  Enablecode39transmit check | 00250  Disable code39transmit check |
| 00280  Disable code39transimit \*  default | 00281  Enable code39transimit\* | 00331  Enable code39Multiple verify |
| 00330  Disable code39Multiple verify default | 02080  Disable  TWO replace 2 in Code 39 | 02081  Enable  TWO replace 2 in Code 39 |
| 01950  Disable code32  Default | 01951  Enable code32  Note:will affect Code39 | 0212M\t  Code39 TABMode |
| 00321  code39Minimum length 1 | 00322  code39 Minimum length 2  Default | 00323  code39 Minimum length 3 |
| 00341  Enable UPC-A  Default | 00340  Disable UPC-A | 0049e  UPC-AIDAs e |
| 00391  Enable UPCAChange to EAN13 | 00390  Disable UPCAChange to EAN13  Default | 00421  Transmit UPCACheck digit  Default |
| 00420  NO-Transmit UPCACheck digit | 00400  UPCADisplay system digit | 00401  UPCAHide system digit |
| 00351  Enable UPC-E  Default | 00350  Disable UPC-E | 0050f  UPCEID As f |
|  | 00381  Enable UPCE Change to UPCA | 00380  Disable UPCE Change to UPCA Default |
| 00361  Enable EAN13  Default | 00360  Disable EAN13 | 0051d  EAN13ID As d |
|  | 00461  Transmit EAN13Check digit  Default | 00460  No-Transmit EAN13Check digit |
|  | 00481  Enable EAN13Change to ISBN | 00480  Disable EAN13Change to ISBNDefault |
|  | 01501  Enable EAN13Change to ISSN | 01500  Disable EAN13Change to ISSN  Default |
|  | 00541  Enable EAN13Multiple verify | 00540  Disable EAN13Multiple verify  Default |
| 00371  Enable EAN8  Default | 00370  Disable EAN8 | 0052c  EAN8IDAs c |
|  | 00571  EAN8 Transmit check digit  Default | 00570  EAN8 No-Transmit check digit |
|  | 00561  EAN8 Hide system digit | 00560  EAN8 display system digit  Default |
| 00552  Enable Fifth digit additional character | 00551  Enable Second digit additional character | 00553  Enable 2nd& 5th digit additional character |
|  |  | 00550  Disable additional character  Default |
| 00621  Enable code93  Default | 00620  Disable code93 | 0066i  code93ID As i |
|  | 00681  Enable code93Multiple verify | 00680  Disable code93Multiple verify  Default |
|  | 01901  Enable Code 93MOD47  Default | 01900  Disable Code 93 MOD47 |
| 00691  Enable code128  Default | 00690  Disable code128 | 0081a  code128ID As a |
|  | 00840  Disable code128 Multiple verify  Default | 00841  Enable code128 Multiple verify |
| 00851  Enable codabar  Default | 00850  Disable codabar | 0094v  codabarID As v |
| 00874  Codabar Minimum length 4 | 00861  Codebar start/stop character tansmission | 00860  Codabartart/stop character without tansmission  Default |
|  | 00951  Enable codabar Multiple verify | 00950  Disable codabar Multiple verify  Default |
| 00961  Enable interleaved 2 of 5  Default | 00960  Disable interleaved 2 of 5 | 0104n  Interleaved 2 of 5ID As n |
| 00974  Interleaved 2 of 5Minimum length 4 | 01050  Disable Interleaved 2 of 5 multiple verify  Default | 01051  Enable Interleaved 2 of 5 multiple verify |
| 01061  Enable industrial 2 of 5  Default | 01060  Disable industrial 2 of 5 | 0113o  Industrial 2 of 5ID As o |
| 01073  Industrial 2 of 5 minimum length 3 | 01141  Enable Industrial 2 of 5 multiple verify | 01140  Disable Industrial 2 of 5 multiple verify  Default |
| 01151  Enable MSI | 01150  Disable MSIDefault | 0053s  MSIID As s |
| 01184  MSI minimum length 4 | 01250  Disable MSI Multiple verify | 01251  Enable MSI Multiple verify Default |
| 01161  Enable Plessey | 01160  Disable Plessey  Default | 0117t  PlesseyID As t |
| 01193  Plessey Minimum length 3 | 01240  Disable PlesseyMultiple verify  Default | 01241  Enable PlesseyMultiple verify |
| 01261  Enable code11  default | 01260  Disable code11 | 0131u  code11ID As u |
| 01284  Code11 Minimum length 4 | 01320  Disable code11 Multiple verify  Default | 01321  Enable code11 Multiple verify |
| 01271  Code11 Auto CK Check | 01272  Code11 C Check  Default | 01273  Code11 CK Check |
| 01461  Enable Matrix 25  Default | 01460  Disable Matrix 25  Default | 00147q  Matrix 25ID As q |
|  | 01482  Matrix 25 Minimum length 2 | 01483  Matrix 25 Minimum length 3 |
| 01571  Enable postal 25 | 01570  Disable postal 25  Default | 0158r  Postal 25ID As r |
|  | 01595  Postal 25 Minimum length 5 | 01597  Postal 25 Minimum length 7 |
| 01871  Enable aerial25 | 01870  Disable aerial25  Default | 0188p  Aerial 25ID Asp |
|  | 01897  Aerial 25 Minimum length 7 |  |
| 01671(only SUC2，CCD)  Enable GS1 Omnidirectional | 01670(only SUC2，CCD)  Disable GS1 Omnidirectional  Default | 0168j(only SUC2，CCD)  GS1 OmniID As j |
| 01771(only SUC2，CCD)  Enable GS1 Limited | 01770(only SUC2，CCD)  Disable GS1 Limited  Default | 0178k(only SUC2，CCD)  GS1 LimitedID As k |
| 01640  FUNC cast light upon cancel  Default | 0160049  FUNC1 Replace with 1 | 0161050  FUNC2 replace with 2 |
|  | 0162051  FUNC3 replace with 3 | 0163054  FUNC4 replace with 4 |
| 0182013  Disable Enter replace  Default | 0182055  Enter replace with 5 |  |
| 0201x  Display Code Front Character  Default | 0200[SPACE]  Hide Code Front Blank |  |
| 0203  Display Code Rear character  Default | 0202[SP]  Hide Code Rear Character |  |
| 0205-  Display Characters inside Code  Default | 0204-  Hide – inside code |  |
| 020600  Disable A replace 0 in code  Default | 02060A  Enable A replace 0 in code |  |
| 02070  Disable One replace 1 in code  Default | 02071  Enable One replace 1 in code |  |
| 02090  Remain character before 12345  Default | 02091  Remove character before 12345 |  |
| 02301  Enable USB fast data upload  Default | 02300  Disable USB fast data upload |  |
| 02311  Enable IR Auto-sensing  Default | 02310  Disable IR Auto-sensing |  |
| 023300  Display rear characters  Default | 023305  Hide rear 5 characters | 023301  Hide rear 1 character |
| 023400  Display front characters | 023405  Hide front 5 characters |  |
| 023900  Display middle characters  Default | 023905  Hide 5 middle characters | 024004  Forward start from 4th character |
| 023530  Trigger timeout 3s  Laser default | 023500  None trigger timeout  CCD default | 023550  Trigger timeout 5s  Laser |
| 02361  All EAN change to ISBN | 02360  Disable EAN change to ISBN  Default |  |
| 02371  All EAN change to ISSN | 02370  Disable EAN change to ISSN  Default |  |
| 02501  Enable upload setting barcodes | 02500  Disable upload setting barcodes  Default |  |
| Wireless Scanner special Settings | | |  | 03010  设置本机地址 |
| 03000  Compulsory pairing （Clear previous pair） | 03001  Pair（None paired device） | 03060  Display stored data quantity |
| 03061  Quantity of available data | 03062  Display receiver address | 03063  Display transmitter address |
| 03011  Dongle Address |  |  |
|  |  |  |
|  | | |  |  |
| Prefix/Suffix Setting | | |  | 0211@[ETX]  所有条码后添加ETX |
| 0212@\r  CR | 0213@\r\n  CR+LF | 0211@[ETX]  All barcodes(rear) add ETX |
| 02160081  All barcodes(front) addF2 | 02110081  All barcodes(rear) addF2 | 0210@  Cancel all barcodes(rear) format character |
| 0217@[STX]  Add STX before barcodes | 0215@  Cancel all boots before barcodes | 02240  Add prefix |
| 02241  Add suffix | 02242  Exit add pre/suffix Mode | 02220  Clear all prefix |
| 02200  Clear all suffix |  |  |
| Character | | |
| 1001  SOH  Note：Used to add Prefix/Suffix | 1002  STX  Note：Used to add Prefix/Suffix | 1003  ETX  Note：Used to add Prefix/Suffix |
| 1004  EOT  Note：Used to add Prefix/Suffix | 1005  ENQ  Note：Used to add Prefix/Suffix | 1006  ACK  Note：Used to add Prefix/Suffix |
| 1007  BEL | 1008  Backspace | 1009  TAB |
| 1010  Line | 1011  VT | 1012  FF |
| 1013  Enter | 1014  SO | 1015  SI |
| 1016  DLE | 1017  DC1 | 1018  DC2 |
| 1019  DC3 | 1020  DC4 | 1021  NAK |
| 1022  SYN | 1023  ETB | 1024  CAN |
| 1025  EM | 1026  SUB | 1027  ESC |
| 1028  FS | 1029  GS | 1030  RS |
| 1031  US | 1032  SPACE | 1033  ! |
| 1034  “ | 1035  # | 1036  $ |
| 1037  % | 1038  & | 1039  ‘ |
| 1040  ( | 1041  ) | 1042  \* |
| 1043  + | 1044  , | 1045  - |
| 1046  . | 1047  / | 1048  0  Note:Used to set  Addrass/prefix/suffix |
| 1049  1  Note:Used to set  Addrass/prefix/suffix | 1050  2  Note:Used to set  Addrass/prefix/suffix | 1051  3  Note:Used to set  Addrass/prefix/suffix |
| 1052  4  Note:Used to set  Addrass/prefix/suffix | 1053  5  Note:Used to set  Addrass/prefix/suffix | 1054  6  Note:Used to set  Addrass/prefix/suffix |
| 1055  7  Note:Used to set  Addrass/prefix/suffix | 1056  8  Note:Used to set  Addrass/prefix/suffix | 1057  9  Note:Used to set  Addrass/prefix/suffix |
| 1058  : | 1059  ; | 1060  < |
| 1061  = | 1062  > | 1063  ? |
| 1064  @ | 1065  A | 1066  B |
| 1067  C | 1068  D | 1069  E |
| 1070  F | 1071  G | 1072  H |
| 1073  I | 1074  J | 1075  K |
| 1076  L | 1077  M | 1078  N |
| 1079  O | 1080  P | 1081  Q |
| 1082  R | 1083  S | 1084  T |
| 1085  U | 1086  V | 1087  W |
| 1088  X | 1089  Y | 1090  Z |
| 1091  [ | 1092  \ | 1093  ] |
| 1094  ^ | 1095  \_ | 1096  ` |
| 1097  a | 1098  b | 1099  c |
| 1100  d | 1101  e | 1102  f |
| 1103  g | 1104  h | 1105  i |
| 1106  j | 1107  k | 1108  l |
| 1109  m | 1110  n | 1111  o |
| 1112  p | 1113  q | 1114  r |
| 1115  s | 1116  t | 1117  u |
| 1118  v | 1119  w | 1120  x |
| 1121  y | 1122  z | 1123  { |
| 1124  | | 1125  } | 1126  ~ |
| 1127  Delete | 1128  F1 | 1129  F2 |
| 1130  F3 | 1131  F4 | 1132  F5 |
| 1133  F6 | 1134  F7 | 1135  F8 |
| 1136  F9 | 1137  F10 | 1138  F11 |
| 1139  F12 | 1140  INSERT | 1141  HOME |
| 1142  Page up | 1143  Delete | 1144  END |
| 1145  Page down | 1146  Right arrow | 1147  Left arrow |
| 1148  Down arrow | 1149  Up arrow |  |
|  |  |  |
| 02510  Disable Change | 02511  All Uppercase | 02512  All lowcase |
| 02513  Uppercase interchange with Lowcase | 02520  Disable long press manage  Note:Wireless scanner not support |  |
| 02530  Disable scan vibrate | 02531  Enable scan vibrate | 02521  Enable long press manage  Note:Wireless scanner not support |
| Wireless Scanner Special Settings | | |
| 03000  Compulsory pairing | 03010  Set scanner address | 000605  Wireless Mode |
| 000607  Auto data save mode | 000606  Inventory mode | 03020  Dongle Add |
|  | 03070  Data Clear | 03050  Resume data upload |
| 03120  Disable beeper when data succeed upload | 03121  Enable beeper when data succeed upload | 03111  Device turn off |
| 0303000 Upload all data and clear | 0303001  Upload 1 data and clear | 0304000  Upload all data and reserve |
| 0304001  Upload 1 data and reserve | 03061  Display quantity of rest data | 0310060  Auto turn off in 60s |
|  |  |  |