|  |  |  |
| --- | --- | --- |
| 000A0Version（custom） | 000A1Display inward character string（custom） | 000A2Display series number（custom） |
| 000B0Factory Default |  | 000600PS2 |
| 000601RS-232 | 000602USB-HID |  |
|  |  |  |
| 013300Default Scan Mode | 013301Single not triggeredNot：CCD inapplicability | 013302Key DelayNo：CCD inapplicability |
| 013303Key Delay not triggeredNot：CCD inapplicability | 013304Continuous Scan Mode | 013305Auto flashing |
| 014201Sound OnDefault | 014200Sound Off |  |
| 014300High Volume Sound | 014301Low Volume Sound |  |
| 01400Code ID Offdefault | 01401Code ID On | 01402Rear Code ID On |
| 0005000EnglishDefault | 0005001Canada-French | 0005002Netherlands-Dutch |
| 0005003Spain-Spanish | 0005004Argentina-Latin American | 0005005Brazil-Portuguese |
| 0005006Denmark-Danish | 0005007UK-English | 0005008Italy-Italian |
| 0005009France-French | 0005010Germany-German | 0005011Norway-Northern Sami |
| 0005012Sweden,Finland-Swedish,Finnish | 0005013Slovakia-Slovak  | 0005014Portuguesa-Portuguese |
| 0005015Czech Republic-Czech | 0005016Belgium -Dutch | 0005017Turkey-F |
| 0005018Turkey-Q | 0005019Poland-Polish | 0005020Switzerland –German,French |
| 0005021Croatia-Srb-Crt | 0005022Hungary -Hungarian | 0005023Japan-Japanese |
| 0005024Russia-Russian |  |  |
| 000701Baudrate600bps | 000702Baudrate1200bps | 000703Baudrate2400bps |
| 000704Baudrate4800bps | 000705Baudrate9600bpsDefault | 000706Baudrate19200bps |
| 000707Baudrate38400bps | 000708Baudrate57600bps | 000709Baudrate115200bps |
| 001200Serial Port no Check | 001201Serial port :XON/OFF | 001202Serial port:RTS/CTS |
| 001203Serial port:ACK/NAK | 0013020Serial port handshake timeout 2S | 0013050Serial port handshake timeout 5S |
| 001500Fastest transmit rate | 001502Medium transmit rate Default | 001504Lower transmit rate |
| 001506Lowest transmit rate | 00161Forward image identifyDefault | 00160Reverse image identify |
| 00221Enable code39 | 00220Disable code39 | 0031mcode39 IDAs m |
| 00231Enable code39FullASCIIDefault | 00230Disable code39 FullASCII | 00240Disable code39 MOD43CheckDefault |
| 00241Enable code39 MOD43Check | 00251Enablecode39transmit check | 00250Disable code39transmit check |
| 00280Disable code39transimit \*default | 00281Enable code39transimit\* | 00331Enable code39Multiple verify |
| 00330Disable code39Multiple verify default | 02080DisableTWO replace 2 in Code 39 | 02081EnableTWO replace 2 in Code 39 |
| 01950Disable code32Default | 01951Enable code32Note:will affect Code39 | 0212M\tCode39 TABMode |
| 00321code39Minimum length 1 | 00322code39 Minimum length 2Default | 00323code39 Minimum length 3 |
| 00341Enable UPC-ADefault | 00340Disable UPC-A | 0049eUPC-AIDAs e |
| 00391Enable UPCAChange to EAN13 | 00390Disable UPCAChange to EAN13Default | 00421Transmit UPCACheck digitDefault |
| 00420NO-Transmit UPCACheck digit | 00400UPCADisplay system digit | 00401UPCAHide system digit |
| 00351Enable UPC-EDefault | 00350Disable UPC-E | 0050fUPCEID As f |
|  | 00381Enable UPCE Change to UPCA | 00380Disable UPCE Change to UPCA Default |
| 00361Enable EAN13Default | 00360Disable EAN13 | 0051dEAN13ID As d |
|  | 00461Transmit EAN13Check digitDefault | 00460No-Transmit EAN13Check digit |
|  | 00481Enable EAN13Change to ISBN | 00480Disable EAN13Change to ISBNDefault |
|  | 01501Enable EAN13Change to ISSN | 01500Disable EAN13Change to ISSNDefault |
|  | 00541Enable EAN13Multiple verify | 00540Disable EAN13Multiple verifyDefault |
| 00371Enable EAN8Default | 00370Disable EAN8 | 0052cEAN8IDAs c |
|  | 00571EAN8 Transmit check digitDefault | 00570EAN8 No-Transmit check digit |
|  | 00561EAN8 Hide system digit | 00560EAN8 display system digitDefault |
| 00552Enable Fifth digit additional character | 00551Enable Second digit additional character | 00553Enable 2nd& 5th digit additional character |
|  |  | 00550Disable additional characterDefault |
| 00621Enable code93Default | 00620Disable code93 | 0066icode93ID As i |
|  | 00681Enable code93Multiple verify | 00680Disable code93Multiple verifyDefault |
|  | 01901Enable Code 93MOD47Default  | 01900Disable Code 93 MOD47 |
| 00691Enable code128Default | 00690Disable code128 | 0081acode128ID As a |
|  | 00840Disable code128 Multiple verifyDefault | 00841 Enable code128 Multiple verify |
| 00851Enable codabarDefault | 00850Disable codabar | 0094vcodabarID As v |
| 00874Codabar Minimum length 4 | 00861Codebar start/stop character tansmission | 00860Codabartart/stop character without tansmissionDefault |
|  | 00951Enable codabar Multiple verify | 00950Disable codabar Multiple verify Default |
| 00961Enable interleaved 2 of 5 Default | 00960Disable interleaved 2 of 5  | 0104nInterleaved 2 of 5ID As n |
| 00974Interleaved 2 of 5Minimum length 4 | 01050Disable Interleaved 2 of 5 multiple verify Default | 01051Enable Interleaved 2 of 5 multiple verify  |
| 01061Enable industrial 2 of 5Default | 01060Disable industrial 2 of 5 | 0113oIndustrial 2 of 5ID As o |
| 01073Industrial 2 of 5 minimum length 3 | 01141Enable Industrial 2 of 5 multiple verify | 01140Disable Industrial 2 of 5 multiple verifyDefault |
| 01151Enable MSI | 01150Disable MSIDefault | 0053sMSIID As s |
| 01184MSI minimum length 4 | 01250 Disable MSI Multiple verify | 01251Enable MSI Multiple verify Default |
| 01161Enable Plessey | 01160Disable PlesseyDefault | 0117tPlesseyID As t |
| 01193Plessey Minimum length 3 | 01240Disable PlesseyMultiple verifyDefault | 01241Enable PlesseyMultiple verify |
| 01261Enable code11default | 01260Disable code11 | 0131ucode11ID As u |
| 01284Code11 Minimum length 4 | 01320Disable code11 Multiple verifyDefault | 01321Enable code11 Multiple verify |
| 01271Code11 Auto CK Check | 01272Code11 C CheckDefault | 01273Code11 CK Check |
| 01461Enable Matrix 25Default | 01460Disable Matrix 25Default | 00147q Matrix 25ID As q |
|  | 01482Matrix 25 Minimum length 2 | 01483Matrix 25 Minimum length 3 |
| 01571Enable postal 25 | 01570Disable postal 25Default | 0158rPostal 25ID As r |
|  | 01595Postal 25 Minimum length 5 | 01597Postal 25 Minimum length 7 |
| 01871Enable aerial25 | 01870Disable aerial25Default | 0188pAerial 25ID Asp |
|  | 01897 Aerial 25 Minimum length 7 |  |
| 01671(only SUC2，CCD)Enable GS1 Omnidirectional | 01670(only SUC2，CCD)Disable GS1 OmnidirectionalDefault | 0168j(only SUC2，CCD)GS1 OmniID As j |
| 01771(only SUC2，CCD)Enable GS1 Limited | 01770(only SUC2，CCD)Disable GS1 LimitedDefault | 0178k(only SUC2，CCD)GS1 LimitedID As k |
| 01640FUNC cast light upon cancelDefault | 0160049FUNC1 Replace with 1 | 0161050FUNC2 replace with 2 |
|  | 0162051FUNC3 replace with 3 | 0163054FUNC4 replace with 4 |
| 0182013Disable Enter replace Default | 0182055Enter replace with 5 |  |
| 0201xDisplay Code Front CharacterDefault | 0200[SPACE]Hide Code Front Blank |  |
| 0203Display Code Rear characterDefault | 0202[SP]Hide Code Rear Character |  |
| 0205-Display Characters inside Code Default | 0204-Hide – inside code |  |
| 020600Disable A replace 0 in codeDefault | 02060AEnable A replace 0 in code |  |
| 02070Disable One replace 1 in codeDefault | 02071Enable One replace 1 in code |  |
| 02090Remain character before 12345Default | 02091Remove character before 12345 |  |
| 02301Enable USB fast data uploadDefault | 02300Disable USB fast data upload |  |
| 02311Enable IR Auto-sensingDefault | 02310Disable IR Auto-sensing |  |
| 023300Display rear charactersDefault | 023305Hide rear 5 characters | 023301Hide rear 1 character |
| 023400Display front characters | 023405Hide front 5 characters |   |
| 023900Display middle charactersDefault | 023905Hide 5 middle characters | 024004Forward start from 4th character |
| 023530Trigger timeout 3sLaser default | 023500None trigger timeoutCCD default | 023550Trigger timeout 5sLaser  |
| 02361All EAN change to ISBN | 02360Disable EAN change to ISBNDefault |  |
| 02371All EAN change to ISSN | 02370Disable EAN change to ISSNDefault |  |
| 02501Enable upload setting barcodes | 02500Disable upload setting barcodesDefault |  |
| Wireless Scanner special Settings |  | 03010设置本机地址 |
| 03000Compulsory pairing （Clear previous pair） | 03001Pair（None paired device） | 03060Display stored data quantity |
| 03061Quantity of available data | 03062Display receiver address | 03063Display transmitter address |
| 03011Dongle Address |  |  |
|  |  |  |
|  |  |  |
| Prefix/Suffix Setting |  | 0211@[ETX]所有条码后添加ETX |
| 0212@\rCR | 0213@\r\nCR+LF | 0211@[ETX]All barcodes(rear) add ETX |
| 02160081All barcodes(front) addF2 | 02110081All barcodes(rear) addF2 | 0210@Cancel all barcodes(rear) format character |
| 0217@[STX]Add STX before barcodes | 0215@Cancel all boots before barcodes | 02240Add prefix |
| 02241Add suffix | 02242Exit add pre/suffix Mode | 02220Clear all prefix |
| 02200Clear all suffix |  |  |
| Character |
| 1001SOHNote：Used to add Prefix/Suffix | 1002STXNote：Used to add Prefix/Suffix | 1003ETXNote：Used to add Prefix/Suffix |
| 1004EOTNote：Used to add Prefix/Suffix | 1005ENQNote：Used to add Prefix/Suffix | 1006ACKNote：Used to add Prefix/Suffix |
| 1007BEL | 1008Backspace | 1009TAB |
| 1010Line | 1011VT | 1012FF |
| 1013Enter | 1014SO | 1015SI |
| 1016DLE | 1017DC1 | 1018DC2 |
| 1019DC3 | 1020DC4 | 1021NAK |
| 1022SYN | 1023ETB | 1024CAN |
| 1025EM | 1026SUB | 1027ESC |
| 1028FS | 1029GS | 1030RS |
| 1031US | 1032SPACE | 1033! |
| 1034“ | 1035# | 1036$ |
| 1037% | 1038& | 1039‘ |
| 1040( | 1041) | 1042\* |
| 1043+ | 1044, | 1045- |
| 1046. | 1047/ | 10480Note:Used to setAddrass/prefix/suffix |
| 10491Note:Used to setAddrass/prefix/suffix | 10502Note:Used to setAddrass/prefix/suffix | 10513Note:Used to setAddrass/prefix/suffix |
| 10524Note:Used to setAddrass/prefix/suffix | 10535Note:Used to setAddrass/prefix/suffix | 10546Note:Used to setAddrass/prefix/suffix |
| 10557Note:Used to setAddrass/prefix/suffix | 10568Note:Used to setAddrass/prefix/suffix | 10579Note:Used to setAddrass/prefix/suffix |
| 1058: | 1059; | 1060< |
| 1061= | 1062> | 1063? |
| 1064@ | 1065A | 1066B |
| 1067C | 1068D | 1069E |
| 1070F | 1071G | 1072H |
| 1073I | 1074J | 1075K |
| 1076L | 1077M | 1078N |
| 1079O | 1080P | 1081Q |
| 1082R | 1083S | 1084T |
| 1085U | 1086V | 1087W |
| 1088X | 1089Y | 1090Z |
| 1091[ | 1092\ | 1093] |
| 1094^ | 1095\_ | 1096` |
| 1097a | 1098b | 1099c |
| 1100d | 1101e | 1102f |
| 1103g | 1104h | 1105i |
| 1106j | 1107k | 1108l |
| 1109m | 1110n | 1111o |
| 1112p | 1113q | 1114r |
| 1115s | 1116t | 1117u |
| 1118v | 1119w | 1120x |
| 1121y | 1122z | 1123{ |
| 1124| | 1125} | 1126~ |
| 1127Delete | 1128F1 | 1129F2 |
| 1130F3 | 1131F4 | 1132F5 |
| 1133F6 | 1134F7 | 1135F8 |
| 1136F9 | 1137F10 | 1138F11 |
| 1139F12 | 1140INSERT | 1141HOME |
| 1142Page up | 1143Delete | 1144END |
| 1145Page down | 1146Right arrow | 1147Left arrow |
| 1148Down arrow | 1149Up arrow |  |
|  |  |  |
| 02510Disable Change | 02511All Uppercase | 02512All lowcase |
| 02513Uppercase interchange with Lowcase | 02520Disable long press manageNote:Wireless scanner not support |  |
| 02530Disable scan vibrate | 02531Enable scan vibrate | 02521Enable long press manageNote:Wireless scanner not support |
| Wireless Scanner Special Settings |
| 03000Compulsory pairing | 03010Set scanner address | 000605Wireless Mode |
| 000607Auto data save mode | 000606Inventory mode | 03020Dongle Add |
|  | 03070Data Clear | 03050Resume data upload |
| 03120Disable beeper when data succeed upload | 03121Enable beeper when data succeed upload | 03111Device turn off |
| 0303000 Upload all data and clear | 0303001Upload 1 data and clear | 0304000Upload all data and reserve |
| 0304001Upload 1 data and reserve | 03061Display quantity of rest data | 0310060Auto turn off in 60s |
|  |  |  |