中文：
------------------------------------------------------------------------------------------
通常DOS环境通过BIOS服务能操作任何串口(INT 14H)和并口(INT 17H)，但是DOS环境里只支持4个串口
(3F8h, 2F8h, 3E8h, 2E8h)和3个并口(3BCh/378h/278h)。

I.文件说明:
1.CH38XDOS.EXE		-- DOS驱动安装工具,支持CH382 2S,2S1P 
2.ReadMe.txt		-- DOS驱动安装工具说明文档

II.选项:
-a			-- 添加CH38X端口
-r			-- CH38X并口重映射到相应的系统保留的端口,只对2S1P的并口起作用
-d			-- 删除添加的CH38X端口
-s			-- 隐藏安装，不提示安装信息
-h			-- 提示安装选项
III.安装步骤:
1. -- 把CH38XDOS通过软驱拷贝到DOS系统. 
2. -- 输入"CH38XDOS"确定是否检测到设备. 
   -- 如果检测到卡会显示: 
  Find CH382 2 Serial 1 Parallel Card
  Serial Port1 at 9000 (IRQ9)
  Serial Port2 at 9400 (IRQ9)
  PrinterPort1 at 9800 (IRQ9)
3. -- 输入"CH38XDOS -a" ,按回车,把CH38XDOS端口安装到系统,显示如下:
  ===========================
  COM1 exists at 3FB
  COM2 exists at 2FB
  COM3 added  at 9000 (IRQ9)
  COM4 added  at 9400 (IRQ9)
  LPT1 exists at 378
  LPT2 added  at 9800 (IRQ9)
  ===========================
4. -- 输入"CH38XDOS -a -r" ,按回车,把CH38XDOS端口安装到系统保留的端口,显示如下:
   ===========================
  COM1 exists at 3FB
  COM2 exists at 2FB
  COM3 added  at 3EB (IRQ9)
  COM4 added  at 2EB (IRQ9)
  LPT1 exists at 378
  LPT2 added  at 278 (IRQ9)
  ===========================
5. -- 如果想每次重启时安装，请在AUTOEXEC.BAT中添加一行:
  CH38XDOS -a -s(或者CH38XDOS -a -r -s)

==========================================================================================

ENGLISH:
------------------------------------------------------------------------------------------
DOS OS operation any serial port (INT 14H) and parallel (INT 17H) by BIOS service commonly,
BUT DOS OS can only support 4 serial port (3F8h, 2F8h, 3E8h, 2E8h) and 3 parallel port
(3BCh/378h/278h).

I. File explain:
1.CH38XDOS.EXE		-- The tool of install the driver support 2S/2S1P/1S1P card for DOS
2.ReadMe.txt		-- The document to explain how to install the driver 

II. Option:
-a			-- Add port of CH38X
-r			-- The por of CH38X remapped to legacy port of DOS OS
-d			-- Delete the add port of CH38X
-s			-- Hidden install, show no install information
-h			-- Clue on install option

III. Install approach:
1. -- Copy the CH38XDOS to DOS OS.
2. -- Input "CH38XDOS" to check the device.
   -- If the card has found, it will display:
  Find CH382 2 Serial 1 Parallel Card
  Serial Port1 at 9000 (IRQ9)
  Serial Port2 at 9400 (IRQ9)
  PrinterPort1 at 9800 (IRQ9)
3. -- Input "CH38XDOS -a", then press "Enter", install the port of CH38XDOS to DOS OS, 
      it will display:
  ===========================
  COM1 exists at 3FB
  COM2 exists at 2FB
  COM3 added  at 9000 (IRQ9)
  COM4 added  at 9400 (IRQ9)
  LPT1 exists at 378
  LPT2 added  at 9800 (IRQ9)
  ===========================
4. -- Input "CH38XDOS -a -r", then press "Enter", install the port of CH38XDOS to legacy
      port of DOS OS, it will display:
  ===========================
  COM1 exists at 3FB
  COM2 exists at 2FB
  COM3 added  at 3EB (IRQ9)
  COM4 added  at 2EB (IRQ9)
  LPT1 exists at 378
  LPT2 added  at 278 (IRQ9)
  ===========================
5. -- If you want install the driver at Reboot every time, please add this line into AUTOEXEC.BAT:
   CH38XDOS -a -s ( or CH38XDOS -a -r -s)
