step1. Install  libusb

 # tar zxvf  libusb-0.1.12.tar.gz 
 # cd libusb-0.1.12                          
 # ./configure                             
 # make                                    
 # make install          ( Login as a root to install driver )          


step2. Install  pcsc-lite
 
 # tar zxvf  pcsc-lite-1.3.2.tar.gz 
 # cd pcsc-lite-1.3.2.tar.gz 
 # ./configure                             
 # make                                    
 # make install          (Login as a root to install driver)
 
step3. Install  ccid driver
 
 # tar zxvf ccid-1.1.0.tar.gz 
 # cd ccid-1.1.0.tar.gz 
 # ./configure                             
 # make                                    
 # make install          (Login as a root to install driver)
 
 step4. Activate the daemon pcscd
 
 #/usr/local/sbin/pcscd
 

 Note:
 	At step2 or step3, when execute the "make" operation .
 	if there has error message - visibility arg must be one of "hidden", "protected" or "internal",
 	solution:
 			replace #define PCSC_API __attribute__ ((visibility("default")))
	 		with       #define PCSC_API 

	At step3, when execute the "./confiure" operation .
	if the error message is  "Package libpcsclite was not found in the pkg-config search path",
 	solution:
 			 Using the following command "PKG_CONFIG_PATH=/usr/local/lib/pkgconfig ./configure"
